The original histogram and the desired histogram of a 64\*64, 3-bit image is given below. Perform histogram specification and do the mapping for the same.

